EOI Concept: Unipole on PPP Model for Akashvani, Siliguri

An EOI (Expression of Interest) for unipole installations under a PPP (Public-Private Partnership) model with All India Radio Siliguri is typically a proposal where a private company has to:

· Install and operate unipole outdoor advertising structures at Akashvani, Siliguri, West Bengal- 734 001 land or premises, 
· Invest for fabrication, erection, maintenance and marketing. 
· Share revenue and 33% of time across all time band with the AIR under a PPP arrangement. 

1. Introduction

Akashvani Siliguri Prasarbharati expresses interest in developing and operating unipole advertisement structures at identified sites belonging to AIR/DD under a Public-Private Partnership (PPP) model.

2. Objective

The objective of this proposal is:

· To utilize available AIR/DD land assets. 
· To develop high-quality unipole advertising. 
· To improve aesthetic and professional outdoor media facilities. 

3. Scope of Work

The proposed private partner shall:

1. Conduct site survey and feasibility assessment, 
2. Design, fabricate, and install unipole structures, 
3. Obtain approvals from local authorities/municipal bodies, 
4. Manage advertising operations, 
5. Ensure structural safety and maintenance, 
6. Share agreed revenue on yearly basis and 33% airtime in all time band with AIR/DD. 
Detailed Scope of Work

1. The SITC of unipole hoardings at the given location along with the operation and maintenance of said unipole.
2. The agency will obtain the right to display the advertisement on LED unipole Street Hoardings after the fulfillment of all clauses laid down in the tender.
3. The agency shall make necessary arrangement to get permissions for Digital Outdoor Advertising and electricity connection from respective Authorities/service providers towards display and illumination of the LED Monopole Street Hoardings and shall bear the necessary charges towards consumption of electricity.
4. The agency will abide by the Advertisement Policy of Prasar Bharati as may be amended from time to time and any such administrative order, circular, notification, G.O. etc. which will come time to time.
5. The agency shall ensure proper electrical and mechanical maintenance of the LED Monopole Street Hoardings and ensure trouble free display at all times, during the tenure of the agreement.
6. Deviation of advertisement area without prior permission of Prasar Bharati will lead to cancellation of the contract with forfeiture of EMD and Security Deposit
7. PRASAR BHARATI shall not be responsible for damage or theft of the frames, structures, flexes, electrical fittings or any other material fixed at the site by the advertiser or for any temporary obstruction caused to the advertisement including pasting of posters etc. by any person/political party. It shall be primary responsibility of the allottee to safeguard and protect their site.
8. The tenure of contract is 05 (five) years from the date of issuance of the work order may be extended for another 5 years  and after completion of the contract period, the right of LED Monopole Street Hoardings to be transferred to the PRASAR BHARATI.

4. Proposed PPP Model

· Private party bears 100% investment cost, 
· Revenue generated from advertisements shall be shared in agreed ratio or in lump- sum on yearly basisalong with 33 % of time in all time band for PB own advertisement. 

5. Proposed Locations

Indicative locations may include:

· Akashvani Bhawan, 2nd Mile, ITI More, Sevoke Road, Dist: Darjeeling, West Bengal – 734001.
· 200 KW DRM MW Transmitter Complex, Akashvani Siliguri, 3rd Mile, Salugara, Sevoke Road, Siliguri-734008.  
 
6. Technical Specifications

Technical Specification 
The technical parameter may change depending on location. The agency may provide the technical specifications, if any change 
	Technical parameters
	Parameter

	LED Make
	M8 Outdoor SMD 2727 Series (GKGD)/Unilumin/Qiangly

	Pixel pitch (mm)
	8

	Pixel density (dots/ m² )
	15625

	Pixel Composition
	1R1G1B

	LED package
	SMD2727

	Module Pixel Density
	40*20

	Module size (mm)
	320*160

	Module Weight(g)
	524.8±2

	Viewing Distance (m)
	≥8m

	Refresh rate (Hz)
	1920

	Module Max. current(A)
	6.6

	Module Max. Power(W)
	33

	Viewing Angle (degree)
	H≥120°V≥120°

	Max. Power(W/ m² )
	645

	Avg. Power (W/ m² )
	322.5

	Brightness (cd/ m² )
	≥4500

	Scan Mode
	1/5 scan, constant current

	Working voltage (V)
	5

	Service Life (h)
	≥100000



	
	Parameter of Outdoor P8 LED Specifications




	 
	LED Full Color Display
	DH80/GKGD/Unilumin/Qiangly

	Module Parameter
	LED Type
	SMD1R1G1B

	
	Pixel Pitch (mm)
	8.0

	
	Module Resolution (W×H)
	40×20

	
	Module Dimension (mm)
	320 (W)×160 (H)

	
	Module Flatness (mm)
	≤0.15

	
	Servicing
	Rear

	
	Back shell
	Plastic

	
	Recommended Cabinet Size
	960×960mm, Metal Folding
(can be customized according to module size)

	Optical Parameter
	Single-dot Brightness Calibration
	Available

	
	Single-dot Color Calibration
	Available

	
	Brightness (nits)
	≥5500

	
	Colour Temperature (K)
	3200—9300 Adjustable

	
	Viewing Angle (Horizontal/Vertical)
	140°

	
	Brightness/Colour Uniformity
	≥97%

	
	Contrast Ratio
	5000:1

	Electrical Parameter
	Max Power Consumption(W/㎡)
	≤810

	
	Average Power Consumption(W/㎡)
	≤270

	
	Input Power Voltage
	AC100-240V, 50/60 (Hz)

	Processing Parameter
	Drive Mode
	Constant Current Drive

	
	Frame Rate (Hz)
	30-120

	
	Refresh Rate (Hz)
	1920-3840

	
	Colour Depth (bits)
	14-16

	Operational
Parameter
	Life span, typ. (Hrs)
	1,00,000

	
	Operating Temp (℃)
	-10—45

	
	Storage Temp (℃)
	-20—60

	
	Operating Humidity (RH)
	10-90%

	
	Storage Humidity (RH)
	10-90%



7. Financial Capability

The company possesses:
· Adequate financial resources, 
· Technical manpower, 
· Experience in outdoor media projects, 
· Vendor network for fabrication and maintenance. 

8. Compliance & Approvals

The bidder/partner shall comply with:
· Municipal advertisement bylaws, 
· Traffic police/NHAI norms, 
· Structural safety certification, 
· Environmental and electrical safety standards. 


9. Documents to be attached

· Company profile, 
· GST registration, 
· PAN card, 
· Experience certificates, 
· Audited financial statements, 
· Previous project photographs, 
· Authorization letter/board resolution. 
· Estimated cost of Unipole




Contact person: 
Amit Lamzel Sarki, Additional Director (Programme), Akashvani, Siliguri, W.B. -734 001
Mob.96792-75787/ email: amitlamzelsarki@prasarbharati.gov.in

The last date for receiving the EOI was on 29/07/2026 (first extension).
However, as no EOI has been received till date, the last date for receiving the EOI is being extended up to 10/08/2026 (second extension). 
	 
(Jiten Kumar Ray, DDGE)
HOO/Cluster Head
Akashvani Siliguri
Mob-94340-61909
